INFORMATION ON NEW TORQUE SPECIFICATIONS. Saturn Saturn 1993

For 1990-2009 cars

# INFORMATION ON NEW TORQUE SPECIFICATIONS

#### SUBJECT: Information on New Torque Specifications

#### MODELS AFFECTED: 1991-1996 Saturns

PURPOSE: Information on new torque specifications at the following joints:

o Steering knuckle-to-strut joint 170 N,m (126 ft-lbs)

o Transaxle strut-to-midrail bolt 70 N,m (52 ft-lbs)

o Engine strut bracket-to-engine bolts 70 N,m (52 ft-lbs)

When servicing the steering knuckle-to strut joint on 1991-1996 Saturns, the new torque specification is 170 N,m (126 ft-lbs).

#### NOTICE: A new steering knuckle-to-strut nut must be used; torque retention of old nut may not be sufficient.

When servicing the transaxle-strut-to-midrail bolt on 1994-1996 Saturns, the new torque specification is 70 N,m (52 ft-lbs).

When servicing the engine strut bracket-to-engine bolts on 1992-1996 Saturns, the new torque specification is 70 N,m (52 ft-lbs).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.