SQUEAKS & RATTLES COMING FROM TOP OR TOP CORNERS. Saturn Saturn 1995

For 1990-2009 cars

# SQUEAKS & RATTLES COMING FROM TOP OR TOP CORNERS

#### SUBJECT: Squeaks and Rattles Coming from Top or Top Corners of Instrument Panel (Check and Repair or Replace Retainers on I/P Upper Trim Panel Outer Corner Filler Assemblies) -------------------------------------------------------------------

#### MODELS AFFECTED: ---------------

1995 Saturn Sedans and Wagons, and 1995-1996 Saturn Coupes

#### CONDITION:

----------

Squeaks and rattles may be coming from the top or top corners of the instrument panel.

#### CAUSE:

------

The squeaks and rattles in the top or top corners of the instrument panel may be caused by I/P upper trim pad retainers (Dual-Lock) losing their adhesion to either the modular dash assembly or the I/P upper trim panel outer corner filler assemblies. Also, the retainers may disengage due to high humidity or heat.

#### CORRECTION:

-----------

Refer to the procedure in this bulletin to remove and replace the I/P upper trim panel outer corner assemblies, and replace any retainers and/or I/P upper trim panel outer corner filler assemblies, if necessary.

#### PROCEDURE

1. Remove I/P upper trim panel outer corner filler assembly, on the side of the vehicle where the squeak or rattle is coming from, by carefully lifting up at the I/P upper trim pad retainers (Dual-Lock) locations.

2. Check retainers to verify that they are securely attached to the modular dash assembly.

3. If any of the retainers are not securely attached to the modular dash assembly:

a. Completely remove retainers that are not securely attached to the modular dash assembly.

b. Thoroughly clean area with Isopropyl alcohol.

c. Replace retainers with new retainers P/N 21040478 .

#### IMPORTANT: Make sure to apply pressure to all four corners and the center of the retainers to ensure proper adhesion to the modular dash assembly.

4. Check retainers to verify that they are securely attached to I/P upper trim panel outer corner filler assembly.

a. If the retainers are not securely attached to the I/P upper trim panel outer corner filler assembly, the I/P upper trim panel outer corner filler assembly must be replaced, since the retainers are sonic welded to the assembly. After new I/P upper trim panel outer corner filler assembly is obtained, proceed to next step.

b. If the retainers are securely attached, proceed to next step.

5. Install I/P upper trim panel outer corner filler assembly and press firmly above where the I/P upper trim pad retainers are, to securely attach to modular dash assembly.

#### PARTS REQUIREMENTS:

21040478 Retainer-I/P Upper Trim Pad 21060433 Filler Asm - I/P Upr T/Pnl Otr Cor (Ebony - LH) 21060434 Filler Asm-I/P Upr T/Pnl Otr Cor (Ebony-RH) 21060435 Filler Asm - I/P Upr T/Pnl Otr Cor (Biscuit - LH) 21060436 Filler Asm - I/P Upr T/Pnl Otr Cor (Biscuit - RH)

#### CLAIM INFORMATION:

To receive credit for this repair during the warranty coverage period, submit a claim through the Saturn Dealer System using the appropriate Electronic Labor Time Guide and Labor Operation Code C2370 (Left Side) and/or C2371 (Right Side

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.