For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the right rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .

1 | Radio Rear Compartment Speaker Refer to Radio Rear Speaker Replacement .
2 | Radio Speaker Amplifier Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 3 N·m (27 lb in)
3 | Radio Speaker Amplifier Assembly

#### Procedure

Disconnect the electrical connector.