For 1990-2009 cars

#### Special Tools

J 41712 Oil Pressure Switch Socket

### Removal Procedure

1. Turn the ignition OFF.
2. Disconnect the oil pressure sensor electrical connector.
3. Remove the oil pressure sensor (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the oil pressure sensor (1).

Tighten
Tighten the oil pressure sensor to 20 N·m (15 lb ft).

2. Connect the oil pressure sensor electrical connector.