For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to SIR Inflator Module Handling and Storage Caution in the Preface section. Caution: A deployed dual stage inflator module will look the same whether one or both stages were used. Always assume a deployed dual stage inflator module has an active stage 2. Improper handling or servicing can activate the inflator module and cause personal injury.

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling .
2. Remove the I/P lower right trim panel. Refer to Instrument Panel Lower Trim Panel Replacement - Right Side .

1 | Instrument Panel Inflatable Restraint Module Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Instrument Panel Upper Trim Panel Assembly Refer to Instrument Panel Upper Trim Panel Replacement .
3 | Instrument Panel Inflatable Restraint Module Assembly Tip:

1. Disconnect the electrical connector.
2. After replacing the module, deploy the old module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling and Scrapping .