For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement .
2. Loosen the seat back cover from the seat back filler panel. It is hooked into the slots of the panel.
3. Slide the rear seat back cover up the seat back enough to gain access to the seat back filler panel screws.

1 | Rear Seat Number 1 Back Panel Screw (Qty: 9) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Rear Seat Number 1 Back Panel