For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Place the ignition switch in the OFF position.
2. Remove the underhood electrical center bracket. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .

1 | Brake Modulator Assembly Bracket Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 20 N·m (15 lb ft)
2 | Brake Modulator Assembly Bracket Nut (Qty: 2) Tighten 10 N·m (89 lb in)
3 | Brake Modulator Assembly Bracket Tip Without disconnecting the brake pipe fittings, carefully remove and support the brake modulator assembly.