For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
2. Disconnect the engine wiring harness electrical connector (4) from the evaporative emission (EVAP) purge solenoid.
3. Disconnect the EVAP pipe quick connect fitting (1) from the EVAP purge solenoid. Refer to Plastic Collar Quick Connect Fitting Service.
4. Disconnect the EVAP pipe quick connect fitting (2) from the EVAP purge solenoid. Refer to Plastic Collar Quick Connect Fitting Service.
5. Remove the EVAP purge solenoid bracket bolt (3).
6. Remove the EVAP purge solenoid.

### Installation Procedure

1. Install the EVAP purge solenoid.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the EVAP purge solenoid bracket bolt (3).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Connect the EVAP pipe quick connect fitting (2) to the EVAP purge solenoid. Refer to Plastic Collar Quick Connect Fitting Service.
4. Connect the EVAP pipe quick connect fitting (1) to the EVAP purge solenoid. Refer to Plastic Collar Quick Connect Fitting Service.
5. Connect the engine wiring harness electrical connector (4) to the EVAP purge solenoid.
6. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.