For 1990-2009 cars

#### Tools Required

J 45053 Universal Clamp Press

1. Remove the front differential transfer drive gear thrust bearing assembly (263) from the front differential transfer drive gear assembly (14).
2. Remove the front differential transfer drive gear thrust bearing washer (264) from the front differential transfer drive gear assembly (14).

Notice: The 4-5 clutch assembly may come out with the front differential transfer drive gear assembly. Do not let the front differential transfer drive gear assembly or the 4-5 clutch assembly fall to the floor or damage may occur.

3. Using J 45053 , remove the front differential transfer drive gear assembly (14) from the transmission case assembly.