For 1990-2009 cars

Condition | Action
--- | ---
Caution: Refer to Hot Exhaust System Caution in the Preface section. DEFINITION: An audible or physical noise due to a faulty component or damaged components causing a loose or misaligned exhaust system resulting in a rattle or vibration noise, i.e. buzz, groan, hum.

Refer to Symptoms - Engine Exhaust prior to beginning this table.

Popping or hissing noise | Exhaust leak - Refer to Exhaust Leakage .
Loud exhaust |

1. Compare to a known good vehicle.
2. Inspect for a damaged or failed muffler or resonator, if equipped.
3. Replace the faulty muffler or resonator (if equipped). Refer to Muffler Replacement .

External rattle or vibration noise |

1. Inspect for a bent or loose hanger, loose heat shield, or loose clamp.
2. Inspect for a exhaust pipe causing interference.
3. Repair or replace the affected component. Refer to the affected component's service procedure.

Internal rattle |

1. Test the components by tapping with a rubber mallet to confirm a rattle.
2. Replace the faulty catalytic converter, resonator, if equipped, or muffler. Refer to Muffler Replacement .