For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tire/wheel assembly. Refer to Tire and Wheel Removal and Installation .

1 | Front Wheelhouse Liner Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 6 N·m (53 lb in)
2 | Front Wheelhouse Liner Bolt Tighten 10 N·m (89 lb in)
3 | Front Wheelhouse Liner Plastic Retainers (Qty: 13)
4 | Front Wheelhouse Liner