For 1990-2009 cars

The following approximate capacities are given in English and metric conversions. See Fluid and Lubricant Recommendations for more information. All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Recheck fluid level after filling.

Application | Specification
--- | ---
Metric | English
Cooling System

- Front Only Climate Control System

10.4 L

11.0 qt

- Front and Rear Climate Control System

11.5 L

12.0 qt

Engine Oil with Filter | 5.2 L | 5.5 qt
Fuel Tank | 70.0 L | 18.5 gal
Automatic Transaxle - AF33-5

- Complete Overhaul

7.8 L

8.2 qt

- Drain and Fill

4.06 L

4.29 qt

Automatic Transmission - 6T70/6T75

- Overhaul

7.0-9.0 L

7.4-9.5 qt

- Drain and Fill

4.0-6.0 L

4.2-6.3 qt

- Valve Body Cover Removal

5.0-7.0 L

5.3-7.4 qt

Rear Axle | 500 ml | 16.9 oz
Transfer Case | 0.8 L | 0.85 qt