For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
2. Remove the rear quarter upper trim panel. Refer to Lock Pillar Upper Garnish Molding Replacement .

1 | Rear Seat Belt Retractor Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tip Apply GM P/N 12345382 (Canadian P/N 10953489), Permatex® 24200 or equivalent on all seat belt fasteners prior to installation. Tighten
45 N·m (33 lb ft)

2 | Rear Seat Belt Retractor Tip Make sure alignment slots are aligned correctly on reinstallation.