For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the left rear trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
2. Disconnect the electrical connector.
3. Calibrate the actuators. Refer to Actuator Recalibration .

1 | Auxiliary Mix Door Actuator Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Auxiliary Mix Door Actuator Tip The mix door actuator is mounted below the air duct outlet side of the module.