For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the hood overslam bumpers. Refer to Hood Bumper Replacement .
2. Remove the primary hood latch. Refer to Hood Primary Latch Replacement .
3. Remove the visible upper bolts for the front headlamps. Refer to Headlamp Replacement .
4. Remove the plastic push pins from the upper fascia as needed. Refer to Front Bumper Fascia Replacement .

1 | Front Bumper Upper Fascia Support Bolts (Qty: 5) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Bumper Upper Fascia Support