For 1990-2009 cars

## Lock Pillar Upper Garnish Molding Replacement Left Side

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
2. Remove rear corner garnish molding. Refer to Body Rear Corner Garnish Molding Replacement .

1 | Lock Pillar Upper Garnish Molding Clip
2 | Lock Pillar Upper Garnish Molding Retainer (Qty: 8)
3 | Lock Pillar Upper Garnish Molding Assembly

## Lock Pillar Upper Garnish Molding Replacement Right Side

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
2. Remove rear corner garnish molding. Refer to Body Rear Corner Garnish Molding Replacement .

1 | Lock Pillar Upper Garnish Molding Clip
2 | Lock Pillar Upper Garnish Molding Retainer (Qty: 9)
3 | Lock Pillar Upper Garnish Molding Assembly