For 1990-2009 cars

The air temperature controls are divided into 4 areas:

• | HVAC control components

• | Heating and A/C operation

• | Engine coolant

• | A/C cycle

### HVAC Control Components

#### HVAC Control Module

The HVAC control module is a non-class 2 device that interfaces between the operator and the HVAC system to maintain air temperature and distribution settings. The battery positive and ignition 1 voltage circuits provide power to the control module. The control module supports the following features:

Feature | Availability
--- | ---
After Blow | Yes
Purge | Yes
Personalization | Yes
Actuator Calibration | Yes

#### Auxiliary HVAC Control Module

The auxiliary HVAC control module is a class 2 device that interfaces between the rear seat occupants and the auxiliary HVAC system to maintain auxiliary air temperature and auxiliary air distribution settings. The battery positive voltage circuit provides power that the control module uses for KAM. If the battery positive voltage circuit loses power, all auxiliary HVAC DTCs and settings will be erased from KAM. The auxiliary HVAC control module will perform a recalibration of the electric actuators when commanded with a scan tool or if KAM is lost. This will ensure the actuators are moving with in the calibrated range.

#### Air Temperature Actuator

The air temperature actuator are 5-wire bi-directional electric motors that incorporate a feedback potentiometer. Low reference, 5-volt reference, position signal, and 2 control circuits enable the actuator to operate. The control circuits use either a 0 or 12-volt value to coordinate the actuator movement. When the actuator is at rest, both control circuits have a value of 0 volts. In order to move the actuator, the HVAC control module grounds one of the control circuits while providing the other with 12 volts. The HVAC control module reverses the polarity of the control circuits to move the actuator in the opposite direction. When the actuator shaft rotates, the potentiometer's adjustable contact changes the door position signal between 0-5 volts.

The HVAC control module uses a range of 0-255 counts to index the actuator position. The door position signal voltage is converted to a 0-255 count range. When the module sets a commanded, or targeted, value, one of the control circuits is grounded. As the actuator shaft rotates the changing position signal is sent to the module. Once the position signal and the commanded value are the same, the module removes power from both control circuits.

#### Auxiliary Air Temperature Actuator

The auxiliary air temperature actuator is a 5-wire bi-directional electric motor that incorporates a feedback potentiometer. Low reference, 5-volt reference, position signal, and 2 control circuits enable the actuator to operate. The control circuits use either a 0 or 12-volt value to coordinate the actuator movement. When the actuator is at rest, both control circuits have a value of 0 volts. In order to move the actuator, the auxiliary HVAC control module grounds one of the control circuits while providing the other with 12 volts. The control module reverses the polarity of the control circuits to move the actuator in the opposite direction. When the actuator shaft rotates, the potentiometers adjustable contact changes the door position signal between 0-5 volts.

The auxiliary HVAC control module uses a range of 0-255 counts to index the actuator position. The door position signal voltage is converted to a 0-255 count range. When the module sets a commanded, or targeted, value, one of the control circuits is grounded. As the actuator shaft rotates, the changing position signal is sent to the module. Once the position signal and the commanded value are the same, the module grounds both control circuits.

#### Air Temperature Sensors

The air temperature sensors are a 2-wire negative temperature co-efficient thermistor. The vehicle uses the following air temperature sensors:

• | Ambient Air Temperature Sensor

• | Inside air temperature sensor assembly

• | Sunload Sensor

• | Upper air temperature sensor

• | Lower air temperature sensor

A signal and low reference circuit enables the sensor to operate. As the air temperature surrounding the sensor increases, the sensor resistance decreases. The sensor signal voltage decreases as the resistance decreases. The sensor operates within a temperature range between -40 to +87.5°C (-40 to +190°F). The sensor signal varies between 0-5 volts.

The input of the duct air temperature sensors are different from the ambient and inside sensors. The HVAC control module converts the signal to a range between 0-255 counts. As the air temperature increases the count value will decrease.

If the HVAC control module detects a malfunctioning sensor, then the control module software will use a defaulted air temperature value. The default value for the inside air temperature sensor will be displayed on the scan tool. The default value for the duct air temperature sensors will not be displayed on the scan tool. The scan tool parameter for the duct air temperature sensors are the actual state of the signal circuit. The default action ensures that the HVAC system can adjust the inside air temperature near the desired temperature until the condition is corrected.

The ambient air temperature sensor mounts underhood and can be affected by city traffic, by idling, and by restarting a hot engine. Therefore, the HVAC control module filters the value of the ambient air temperature sensor for temperature display. The ambient air temperature value is updated under the following conditions:

Condition | Display
--- | ---
When the HVAC module A/C and RECIRCULATION buttons are pressed simultaneously. | Updates temperature display instantly
At start up with the engine off less than 2 hours | Displays last stored temperature unless temperature has decreased. The outside air temperature reading is always instantly updated if ambient air temperature has decreased.
At start up with the engine off more than 2 hours | Displays actual outside temperature
Vehicle speed above 32 km/h (20 mph) for a minimum of 80 seconds | Updates temperature display at a slow filtered rate
Sensor ambient temperature reading is less than the last displayed value | Displays actual outside temperature
When the ambient air decreases. | Updates temperature display rapidly

#### Sunload Sensor

The sunload sensor is a 2-wire photo diode. The vehicle uses left and right sunload sensors. The 2 sensors are integrated into the sunload sensor assembly. Low reference and signal circuits enable the sensor to operate. As the light shining upon the sensor gets brighter, the sensor resistance increases. The sensor signal decreases as the resistance increases. The sensor operates within an intensity range between completely dark and bright. The sensor signal varies between 0-5 volts. The HVAC control module converts the signal to a range between 0-255 counts.

The sunload sensor provides the HVAC control module a measurement of the amount of light shining on the vehicle. Bright, or high intensity, light causes the vehicles inside temperature to increase. The HVAC system compensates for the increased temperature by diverting additional cool air into the vehicle.

If the HVAC control module detects a malfunctioning sensor, then the control module software will use a defaulted sunload value. This value will not be displayed on the scan tool. The default action ensures that the HVAC system can adjust the inside air temperature near the desired temperature until the condition is fixed. The scan tool parameter for the sunload sensor is the actual state of the signal circuit.

#### A/C Refrigerant Pressure Sensor

The A/C refrigerant pressure sensor is a 3-wire piezoelectric pressure transducer. A 5-volt reference, low reference, and signal circuits enable the sensor to operate. The A/C pressure signal can be between 0-5 volts. When the A/C refrigerant pressure is low, the signal value is near 0 volts. When the A/C refrigerant pressure is high, the signal value is near 5 volts.

The A/C refrigerant pressure sensor protects the A/C system from operating when an excessively high or low pressure condition exists. The engine control module (ECM) disables the compressor clutch under the following conditions:

• | The A/C high side pressure is more than 2,929 kPa (425 psi).

• | The clutch will be enabled after the high side pressure decreases to less than 1,376 kPa (200 psi).

• | A/C low side pressure is less than 269 kPa (39 psi).

• | The clutch will be enabled or will allow engagement again after the low side pressure increases to more than 296 kPa (43 psi).

#### Evaporator Low Ambient Protection

The refrigerant temperature at the temperature sensor on the evaporator case controls cycling of the compressor clutch to prevent freezing of the evaporator core. The compressor is disabled when the temperature goes below 3°C (37°F) and vehicle speed is greater than 8 km/h (5 mph). The compressor is enabled when the temperature exceeds 4°C (40°F). The minimum cycling time off is 4 seconds.

#### Heating and A/C Operation

The purpose of the heating and A/C system is to provide heated and cooled air to the interior of the vehicle. The A/C system will also remove humidity from the interior and reduce windshield fogging. The vehicle operator can determine the passenger compartment temperature by adjusting the air temperature control. Regardless of the temperature setting, the following can effect the rate that the HVAC system can achieve the desired temperature:

• | Recirculation

• | Difference between inside and desired temperature

• | Difference between ambient and desired temperature

• | Blower motor speed setting

• | Mode setting

The vehicle operator can activate the A/C system by pressing the A/C switch. The A/C system can operate regardless of the temperature setting.

The engine control module (ECM) will operate the A/C system automatically in FRONT DEFROST mode to help reduce moisture inside the vehicle. The A/C LED will not illuminate unless the driver presses the A/C request switch on the HVAC control module. The A/C system maybe running without the A/C LED indicator illuminated when in FRONT DEFROST mode. The HVAC system uses a compressor that incorporates a thermal switch that opens once the compressor temperature exceeds 211-217°C (380-454°F) creating an open circuit. The following conditions must be met in order for the ECM to turn on the compressor clutch:

• | BCM

- | Battery voltage between 11-16 volts

- | A/C request from the HVAC control module

• | ECM

- | Engine coolant temperature (ECT) is greater than 117°C (243°F).

- | Engine speed is less than 4,760 RPM.

- | A/C pressure is between 2,929-2,706 kPa (425-39 psi).

Once engaged, the compressor clutch will be disengaged for the following conditions:

• | Throttle position is 100 percent

• | A/C pressure is more than 2,929 kPa (425 psi).

• | A/C pressure is less than 269 kPa (39 psi).

• | ECT is more than 120°C (248°F).

• | Engine speed is more than 6240 RPM.

• | Transmission shift

• | ECM detects excessive torque load.

• | ECM detects insufficient idle quality.

• | ECM detects a hard launch condition.

When the compressor clutch disengages, the compressor clutch diode protects the electrical system from a voltage spike.

#### Engine Coolant

Engine coolant is the key element of the heating system. The thermostat controls engine operating coolant temperature. The thermostat also creates a restriction for the cooling system that promotes a positive coolant flow and helps prevent cavitation. Coolant enters the heater core through the inlet heater hose, in a pressurized state.

The heater core is located inside the HVAC module. The heat of the coolant flowing through the heater core is absorbed by the ambient air drawn through the HVAC module. Heated air is distributed to the passenger compartment, through the HVAC module, for passenger comfort.

The amount of heat delivered to the passenger compartment is controlled by opening or closing the HVAC module air temperature door. The coolant exits the heater core through the return heater hose and recirculated back through the engine cooling system.

### A/C Cycle

Refrigerant is the key element in an air conditioning system. R-134a is presently the only EPA approved refrigerant for automotive use. R-134a is a very low temperature gas that can transfer the undesirable heat and moisture from the passenger compartment to the outside air.

The A/C compressor is belt driven and operates when the magnetic clutch is engaged. The compressor builds pressure on the vapor refrigerant, which adds heat to the refrigerant. The refrigerant is discharged from the compressor, through the discharge hose, and forced to flow to the condenser and then through the balance of the A/C system. The A/C system is mechanically protected with the use of a high pressure relief valve. If the high pressure switch were to fail or if the refrigerant system becomes restricted, and the refrigerant pressure continues to rise, the high pressure relief valve will pop open and release refrigerant from the system.

Compressed refrigerant enters the condenser in a high temperature, high pressure vapor state. As the refrigerant flows through the condenser, the heat of the refrigerant is transferred to the ambient air passing through the condenser. Cooling the refrigerant causes the refrigerant to condense and change from a vapor to a liquid state.

The condenser is located in front of the radiator for maximum heat transfer. The condenser is made of aluminum tubing and aluminum cooling fins, which allows rapid heat transfer for the refrigerant. The semi-cooled liquid refrigerant exits the condenser and flows through the liquid line, to the thermal expansion valve (TXV).

The TXV is located at the evaporator inlet and outlet pipes. The TXV is the dividing point for the high and the low pressure sides of the A/C system. As the refrigerant passes through the TXV, the pressure on the refrigerant is lowered. Due to the pressure differential on the liquid refrigerant, the refrigerant will begin to boil at the TXV. The TXV also meters the amount of liquid refrigerant that can flow into the evaporator.

Refrigerant exiting the TXV flows into the evaporator core in a low pressure, liquid state. Ambient air is drawn through the HVAC module and passes through the evaporator core. Warm and moist air cause the liquid refrigerant to boil inside of the evaporator core. The boiling refrigerant absorbs heat from the ambient air and draws moisture onto the evaporator. The refrigerant exits the evaporator through the suction line and back to the compressor, in a vapor state, and completing the A/C cycle of heat removal. At the compressor, the refrigerant is compressed again and the cycle of heat removal is repeated.

The conditioned air is distributed through the HVAC module for passenger comfort. The heat and moisture removed from the passenger compartment condense, and is discharged from the HVAC module as water.