For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Disable the SIR. Refer to SIR Disabling and Enabling .
2. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement .
3. Remove ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement

1 | Theft Deterrent Module Assembly

#### Procedure

1. Disconnect electrical connectors.
2. Program theft deterrent control module after replacement. Refer to Control Module References