For 1990-2009 cars

### Calibration Criteria

The brake pedal position sensor (BPPS) receives a low reference signal and a 5-volt reference signal from the BCM. Whenever the brake pedal is applied, the BPPS applies a variable voltage signal to the BCM through the stop lamp switch signal circuit. The BPPS calibration must be performed after the BPPS or body control module (BCM) have been serviced. The calibration procedure will set BPPS home value. This value is used by the BCM to determine the action of the driver applying the brake system and to provide this information to the vehicle subsystems via the communication bus.

### Calibration Procedure

• | Install a scan tool.

• | Turn ON the ignition, with the engine OFF.

• | Select Diagnostics.

• | Select the year.

• | Select the vehicle type.

• | Select BCM.

• | Select Module Setup.

• | Select the BPPS calibration procedure and follow the directions displayed on the screen.