For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .

1 | Rear Side Door Window Frame Rear Applique Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Rear Side Door Window Frame Rear Applique Clip Tip: Replace the clip if damaged, transfer the clip to the new part.
3 | Rear Side Door Window Frame Rear Applique