For 1990-2009 cars

1. Remove the right exhaust manifold heat shield bolts.
2. Remove the right exhaust manifold heat shield.
3. Remove the right exhaust manifold bolts from the right cylinder head.
4. Remove the right exhaust manifold nuts from the studs in the right cylinder head.
5. Remove the right exhaust manifold.
6. Remove and discard the right exhaust manifold gasket.
7. Remove the studs from the right cylinder head.