For 1990-2009 cars

### Removal Procedure

1. It is only necessary to lower the headliner. Only do those step in headliner replacement that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement .
2. Depress the tab on the side of the control module.
3. With the tab depressed, slide the sunroof control module toward the sunroof motor. This will release the control module from the sunroof module.
4. Remove the control module from the sunroof module and disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector to the sunroof control module.
2. Insert the control module tabs into the sunroof module slots.
3. Slide the sunroof express module away from the sunroof motor until it is fully engaged.
4. Verify the proper operation of the sunroof before securing the headliner.
5. Install the headliner. Refer to Headlining Trim Panel Replacement .