For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Lower the rear of the headliner. Refer to Headlining Trim Panel Replacement .

1 | Digital Radio Coaxial Cable

#### Procedure

1. Disconnect all electrical/antenna connections.
2. When the original antenna is wrapped in the vehicle wiring harness perform the following steps:

• | Cut both ends off the original antenna cable.

• | Route the new antenna next to the vehicle wiring harness and secure with tie straps.