For 1990-2009 cars

### Removal Procedure

Note: The EVAP emissions canister is located under the center of the vehicle. It has 3 EVAP line connections:

• | The EVAP fresh air

• | The EVAP vent

• | The EVAP purge

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Caution: Clean all fuel pipe connections and surrounding areas before disconnecting the fuel pipes to avoid contamination of the fuel system.

2. Disconnect the EVAP canister fresh air hose/pipe from the fuel tank fresh air hose/pipe (2). Refer to Plastic Collar Quick Connect Fitting Service.
3. Disconnect the EVAP canister vent hose/pipe from the EVAP canister. Refer to Plastic Collar Quick Connect Fitting Service.
4. Disconnect the EVAP canister purge hose/pipe (1) from the EVAP canister.
5. Remove the EVAP canister-to-underbody nuts (3).
6. Lower the EVAP canister.
7. Disconnect the EVAP vent solenoid electrical connector (1).
8. Remove the EVAP canister (4) from the vehicle.

### Installation Procedure

1. Connect the EVAP vent solenoid electrical connector (1).
2. Install the EVAP canister (4) to the underbody of the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the EVAP canister-to-underbody nuts (3) tightening the nuts to 9 N·m (80 lb in).
4. Connect the EVAP canister purge hose/pipe (1) to the EVAP canister.
5. Connect the EVAP canister vent hose/pipe (3) to the EVAP canister. Refer to Plastic Collar Quick Connect Fitting Service.
6. Connect the EVAP canister fresh air hose/pipe to the fuel tank fresh air hose/pipe (2). Refer to Plastic Collar Quick Connect Fitting Service.
7. Lower the vehicle.