For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Loosen the stabilizer shaft clamp bolts.

Important: Use a 90° bend TORX® bit to hold the ball stud when loosening or tightening the nut.

4. Remove the stabilizer link to stabilizer shaft nut.

Important: When disconnecting the stabilizer link, hold the link with a wrench to prevent turning.

5. Remove the stabilizer link to lower control arm nut.
6. Remove the stabilizer link from the vehicle.

### Installation Procedure

1. Position the stabilizer link through the lower control arm.

Notice: Refer to Fastener Notice in the Preface section.

Important: When connecting the stabilizer link, hold the link with a wrench to prevent turning.

2. Install the stabilizer link to lower control arm nut.

Tighten
Tighten the nut to 15 N·m (11 lb ft).

Important: Use a 90° bend TORX® bit to hold the ball stud when tightening the nut.

3. Install the stabilizer link to stabilizer shaft nut.

Tighten
Tighten the nut to 50 N·m (37 lb ft).

4. Tighten the loose stabilizer shaft clamp bolts.

Tighten
Tighten the bolts to 70 N·m (52 lb ft).

5. Install the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
6. Lower the vehicle.