For 1990-2009 cars

1. Install the park pawl pin spring (704).
2. Install the park pawl pin spring guide sleeve (705).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the park pawl bolt/screw (706).

Tighten
Tighten the park pawl bolt to 10 N·m (89 lb in).

4. Install the park pawl spring pin (703).
5. Install the park pawl (702) and the park pawl actuator bracket (708).
6. Install the park pawl return spring (701).
7. Install the park pawl shaft (700).
8. Install the manual shift detent spring assembly (711).
9. Install and hand tighten the 14 mm manual shift detent lever spring bolt (712) and the 16.7 mm park pawl actuator bracket bolt (715).

Tighten

• | Tighten the 14 mm manual shift detent lever spring bolt (712) to 5 N·m (44 lb in).

• | Tighten the 16.7 mm park pawl actuator bracket bolt (715) to 10 N·m (89 lb in).

10. Install the park pawl actuator rod (709).
11. Install the manual shift detent lever assembly (710).

Important: The park pawl actuator rod (709) must be installed with the rod between the case and the manual shift detent lever.

12. Connect the park pawl actuator rod (709) to the manual shift detent lever assembly (710).
13. Using a screwdriver, lift the manual shift detent lever spring (711) and rotate the manual shift detent lever assembly (710) into position.