For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the rear side door water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Disconnect the electrical connector from the rear side door window regulator motor.
4. Remove the rear side door window regulator motor to regulator screws.
5. Remove the rear side door window regulator motor.

### Installation Procedure

1. Align the rear side door window regulator motor to the rear side door window regulator.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear side door window regulator motor to regulator screws.

Tighten
Tighten to 8 N·m (71 lb in).

3. Connect the electrical connector to the rear side door window regulator motor.
4. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement .
5. Install the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .