For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging
2. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
3. Remove the rubber exhaust hangers to gain access to the auxiliary A/C and the 3 heater pipes.
4. Remove the auxiliary air conditioning (A/C) lines from the thermal expansion valve (TXV).

1 | Thermal Expansion Valve (TXV) Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3.5 N·m (31 lb in)
2 | Thermal Expansion Valve (TXV) - Auxiliary Tip If the TXV mounting block needs servicing, the auxiliary EVAP core must be removed
3 | Sealing Washer (Qty: 2) Tip Remove and discard the sealing washer. Refer to Sealing Washer Replacement.