For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Box Bolt | 20 N·m | 15 lb ft
Battery Hold Down Bolt | 15 N·m | 11 lb ft
Battery Negative Cable Terminal Bolt | 17 N·m | 13 lb ft
Battery Positive Cable Terminal Bolt | 17 N·m | 13 lb ft
Battery Tray Support Bracket Bolt | 25 N·m | 18 lb ft
Generator Battery Positive Terminal Nut | 20 N·m | 15 lb ft
Generator Bolt | 50 N·m | 37 lb ft
Negative Battery Cable to Wheelhouse Stud Nut | 12 N·m | 106 lb in
Negative Battery Cable to Transaxle Nut | 45 N·m | 33 lb ft
Starter Bolt | 50 N·m | 37 lb ft
Starter Solenoid Positive Battery Terminal Nut | 10 N·m | 89 lb in
Under Hood Fuse Block (UHFB) Battery Positive Terminal Nut | 15 N·m | 11 lb ft