For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
2. Remove the floor console. Refer to Console Replacement.

1 | Inflatable Restraint Vehicle Rollover Sensor Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Inflatable Restraint Vehicle Rollover Sensor Assembly

#### Procedure

Disconnect the electrical connectors.

Tip
Position the carpet in order to access the sensor.