For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liners. Refer to Front Wheelhouse Liner Replacement .

1 | Front Bumper Fascia Plastic Retainer (Qty: 5)
2 | Front Bumper Fascia Plastic Retainer (Qty: 6)
3 | Front Bumper Fascia

#### Procedure

1. Disconnect all electrical connectors.
2. Use a pry tool to release the fascia retaining tabs from the fascia lower support.