For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
2. Support the engine. Refer to Engine Support Fixture .
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
4. Remove three engine mount bracket bolts (1).
5. Remove engine mount bracket to engine mount bolt.
6. Remove engine mount from vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Position engine mount in place and install engine mount bracket to engine mount bolt.

Tighten
Tighten the bolt to 50 N·m (37 lb ft).

2. Install the engine mount to frame bolts (1).

Tighten
Tighten the engine mount bolts to 50 N·m (37 lb ft).

3. Lower the vehicle.
4. Remove the engine support. Refer to Engine Support Fixture .
5. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .