For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Front Seat Replacement - Bucket .

1 | Front Seat Recliner Handle Tip Pull firmly forward on the handle to remove.
2 | Front Seat Outer Adjuster Finish Cover Refer to Front Seat Cushion Outer Trim Panel Replacement .
3 | Front Seat Belt Buckle Refer to Front Seat Belt Buckle Replacement .
4 | Front Seat Inner Adjuster Finish Panel Refer to Front Seat Cushion Inner Trim Panel Replacement .
5 | Front Seat Lumbar Support Actuator Knob

#### Procedure

1. Adjust the lumbar knob until the lumbar is in the setting of the least support.
2. Remove the lumbar knob by pulling firmly away from the seat.

6 | Front Seat Cushion Cover

#### Procedure

1. Remove the seat cushion frame bolts and seat cushion assembly from the seat.
2. Disconnect the J-hook retainers.
3. Disengage the J-strip at the rear of the cushion.
4. Remove the seat cushion cover from the pad by carefully disengaging the hook and loop retainers.

7 | Front Seat Cushion Pad

#### Procedure

Disconnect the electrical connector, if equipped.