For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the liftgate in order to access the tail lamp access hole covers and screws.

1 | Tail Lamp Access Hole Cover Assembly (Qty: 2)
2 | Tail Lamp Screws (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten Tighten the screws in the sequence shown to 2.5 N·m (22 lb in)
3 | Tail Lamp Assembly Tip Pull the lamp assembly rearward, disengage the locator pins and disconnect the electrical connector.
4 | Tail Lamp Locator Pins (Qty: 2) Tip Use palm pressure to engage the locator pins to quarter panel upon re-installation of the tail lamp.
5 | Rear Quarter Panel Nuts (Qty: 2)