For 1990-2009 cars

#### Fastener Tightening Specifications

Description of Usage | Ref No.* | Qty | Size | Specification
--- | --- | --- | --- | ---
Metric | English
Automatic Transmission Fluid Pump (2) to Transmission Case Assembly (17) | 5 | 8 | M8x1.25x28 mm | 25 N·m | 18 lb ft
Battery Negative Cable and Wire Harness Ground to Transaxle Stud Nut | -- | -- | -- | 45 N·m | 33 lb ft
Control Valve Body Cover (29) to Transmission Case Assembly (17) | 28 | 9 | M8x1.25x15.5 mm | 13 N·m | 10 lb ft
Control Valve Body Fluid Passage Cover (37) to Control Valve Body (39) | 30 | 2 | M6x1.0x55 mm | 10 N·m | 89 lb in
Fluid Baffle (803) to Torque Converter Housing Assembly (801) | 807 | 3 | M6x1.0x14 mm | 5 N·m | 44 lb in
Fluid Baffle (803) to Transmission Case Assembly (17) | 45 | 3 | M6x1.0x14.7 mm | 5 N·m | 44 lb in
Fluid Baffle (830) to Transmission Case Assembly (17) | 829 | 2 | M6x1.0x12 mm | 5 N·m | 44 lb in
Fluid Filter (42) to Transmission Case (17) | 43 | 1 | M6x1.0x16.7 mm | 5 N·m | 44 lb in
Fluid Level Indicator Bolt | 825 | 1 | M8x1.25x25 mm | 10 N·m | 89 lb in
Fluid Pump Body (202) to Fluid Pump Stator Shaft Assembly (208) | 231 | 13 | M6x1.0x14.5 mm | 12 N·m | 106 lb in
Fluid Pump Body (202) to Fluid Pump Stator Shaft Assembly (208) | 232 | 1 | M5x0.8x17 mm | 7 N·m | 62 lb in
Fluid Temperature Sensor Clip (49) to Control Valve Body (39) | 31 | 1 | M6x1.0x50 mm | 10 N·m | 89 lb in
Forward Clutch Accumulator Cover (616) to Case Cover (606) | 617 | 2 | M6x1.0x14.5 mm | 10 N·m | 89 lb in
Front Transaxle Mount (2) and Transaxle Bolts | -- | -- | -- | 90 N·m | 66 lb ft
Fuel Line Retaining Clip Nut | -- | -- | -- | 25 N·m | 18 lb in
Lower 4 Transaxle to Engine Bolts | -- | -- | -- | 75 N·m | 55 lb ft
Lube Fluid Pipe Retainer (805) to Torque Converter Housing (801) | 806 | 1 | M6x1.0x14 mm | 5 N·m | 44 lb in
Lube Fluid Pipe Retainer (84) to Transmission Case Assembly (17) | 83 | 1 | M6x1.0x19.5 mm | 5 N·m | 44 lb in
Manual Shift Detent Spring (711) to Transmission Case (707) | 712 | 1 | M6x1.0x14 mm | 5 N·m | 44 lb in
Park Pawl Actuator Bracket (708) to Transmission Case Assembly (17) | 715 | 1 | M6x1.0x16.7 mm | 10 N·m | 89 lb in
Park Pawl Bolt/Screw (706) to Transmission Case Assembly (17) | 706 | 1 | M6x1.0x25 mm | 10 N·m | 89 lb in
Rear Valve Body Cover Plate Bolt - Hexagon | 416 | 2 | M5x0.8x13 mm | 7 N·m | 62 lb in
Rear Valve Body Cover Plate Bolt - Hexagon | 421 | 7 | M5x0.8x13 mm | 7 N·m | 62 lb in
Securing the Battery Negative Cable and Wire Harness Ground to Transaxle Stud | -- | -- | -- | 45 N·m | 33 lb ft
Shift Control Knob Screw | -- | -- | -- | 1.5 N·m | 13 lb in
Shift Control Nuts | -- | -- | -- | 25 N·m | 18 lb ft
Speed Sensor (73) to Transmission Case Assembly (17) | 61 | 2 | M6x1.0x16 mm | 5 N·m | 44 lb in
Stabilizer Link Nuts | -- | -- | -- | 65 N·m | 48 lb ft
Torque Converter Housing (10) to Transmission Case Assembly (17) | 3 | 1 | M8x1.25x30 mm | 29 N·m | 21 lb ft
Torque Converter Housing (10) to Transmission Case Assembly (17) | 4 | 12 | M8x1.25x30 mm | 29 N·m | 21 lb ft
Torque Converter Housing (10) to Transmission Case Assembly (17) | 6 | 2 | M8x1.25x35 mm | 29 N·m | 21 lb ft
Torque Converter Housing (10) to Transmission Case Assembly (17) | 7 | 1 | M8x1.25x45 mm | 29 N·m | 21 lb ft
Torque Converter Housing (10) to Transmission Case Assembly (17) - TORX | 8 | 1 | M8x1.25x30 mm | 29 N·m | 21 lb ft
Torque Converter to Flywheel Bolts | -- | -- | -- | 60 N·m | 44 lb ft
Transaxle Brace Bolts | -- | -- | -- | 50 N·m | 37 lb ft
Transaxle Control Bracket Nuts | -- | -- | -- | 25 N·m | 18 lb ft
Transaxle Front Mount Bolts | -- | -- | -- | 90 N·m | 66 lb ft
Transaxle Left Mount Nuts | -- | -- | -- | 37 N·m | 27 lb ft
Transaxle Mount to Bracket Bolts | -- | -- | -- | 55 N·m | 41 lb ft
Transaxle Mount to Bracket Bolts | -- | -- | -- | 37 N·m | 27 lb ft
Transaxle Mount to Bracket Nuts | -- | -- | -- | 37 N·m | 27 lb ft
Transaxle Oil Cooler Line Assembly Nut at the Transaxle | -- | -- | -- | 9 N·m | 80 lb in
Transaxle Range Selector Lever Nut | -- | -- | -- | 16 N·m | 12 lb ft
Transaxle Rear Mount Bracket Bolts | -- | -- | -- | 55 N·m | 41 lb ft
Transaxle Rear Mount Bracket Bolts | -- | -- | -- | 37 N·m | 27 lb ft
Transaxle Shift Control Cable Bracket Bolts | -- | -- | -- | 25 N·m | 18 lb ft
Transaxle to Engine Bolts | -- | -- | -- | 75 N·m | 55 lb ft
Transmission Case Cover (606) to Transmission Case Assembly (17) | 74 | 1 | M8x12.5x30 mm M6x1.0x10 mm | 25 N·m | 18 lb ft
Transmission Case Cover (606) to Transmission Case Assembly (17) | 77 | 1 | M8x1.25x72 mm | 25 N·m | 18 lb ft
Transmission Case Cover (606) to Transmission Case Assembly (17) | 20 | 8 | M8x1.25x30 mm | 25 N·m | 18 lb ft
Transmission Case Cover (606) to Transmission Case Assembly (17) | 21 | 1 | M8x1.25x48 mm | 25 N·m | 18 lb ft
Transmission Case Cover (606) to Transmission Case Assembly (17) | 22 | 2 | M8x1.25x45 mm | 25 N·m | 18 lb ft
Transmission Case Fluid Passage Cover (40) to Transmission Case Assembly (17) | 41 | 2 | M6x1.0x14 mm | 5 N·m | 44 lb in
Transmission Control Module (TCM) Bolts | 76 | 3 | M6x1.0x16 mm | 25 N·m | 18 lb ft
Transmission Fluid Drain Plug (819) to Torque Converter Housing (801) | 819 | 1 | M18x12 mm | 39 N·m | 29 lb ft
Transmission Fluid Pressure Test Hole Plug | 66 | 9 | -- | 7 N·m | 62 lb in
Transmission Front Mount Thru Bolt | -- | -- | -- | 110 N·m | 81 lb ft
Transmission Left Mount Bracket Bolts | -- | -- | -- | 55 N·m | 41 lb ft
Transmission Mount Bracket Bolts | -- | -- | -- | 55 N·m | 41 lb ft
Transmission Mount to Bracket Thru Bolt | -- | -- | -- | 110 N·m | 81 lb ft
Transmission Mount to Frame Bolts | -- | -- | -- | 50 N·m | 37 lb ft
Transmission Rear Mount Bolts | -- | -- | -- | 50 N·m | 37 lb ft
Transmission Rear Mount Thru Bolts | -- | -- | -- | 110 N·m | 81 lb ft
Upper 4 Transaxle to Engine Bolts | -- | -- | -- | 75 N·m | 557 lb ft
3rd Gear Band Anchor Bolt (64) to Transmission Case Assembly (17) | 64 | 1 | M20x1.5x21 mm | 167 N·m | 123 lb ft
3rd Gear Band Apply Tube Retainer (51) to Transmission Case Assembly (17) | 50 | 2 | M6x1.0x14 mm | 5 N·m | 44 lb in
4-5 Clutch Apply Pipe Retainer (610) to Transmission Case Cover (606) | 611 | 4 | M5x0.8x12 mm | 7 N·m | 62 lb in
Valve Body

- Control Valve Body (39) to Transmission Case Assembly (17)

34

2

M6x1.0x16 mm

10 N·m

89 lb in

- Control Valve Body (39) to Transmission Case Assembly (17)

35

2

M6x1.0x50 mm

10 N·m

89 lb in

- Control Valve Body (39) to Transmission Case Assembly (17)

47

3

M6x1.0x55 mm

10 N·m

89 lb in

- Control Solenoid Valve Retainer (312) to Control Valve Body (39)

311

1

M5x0.8x13 mm

7 N·m

62 lb in

- Front Control Valve Body (315) to Middle Control Valve Body (323)

313

5

M5x0.8x20 mm

7 N·m

62 lb in

- Front Control Valve Body (315) to Middle Control Valve Body (323)

314

2

M5x0.8x16 mm

7 N·m

62 lb in

- Front Control Valve Body (315) to No. 2 Rear Control Valve Body (330)

331

1

M5x0.8x76 mm

7 N·m

62 lb in

- Front Control Valve Body (315) to No. 2 Rear Control Valve Body (330)

332

4

M5x0.8x49.5 mm

7 N·m

62 lb in

- Lock Up Control Solenoid Valve (339) to Front Control Valve Body (315)

307

1

M5x0.8x10 mm

7 N·m

62 lb in

- Middle Control Valve Body (323) Pressure Tap

334

1

M6x1.0x12 mm

7 N·m

62 lb in

- Middle Control Valve Body (323) to No. 2 Rear Control Valve Body (330)

304

1

M5x0.8x50 mm

7 N·m

62 lb in

- No. 2 Rear Control Valve Body (330) to Front Control Valve Body (315)

304

1

M5x0.8x50 mm

7 N·m

62 lb in

- Rear Control Valve Body (326) to Middle Control Valve Body (323)

333

1

M5x0.8x40 mm

7 N·m

62 lb in

- Rear Control Valve Body (326) to Middle Control Valve Body (323)

335

2

M5x0.8x35 mm

7 N·m

62 lb in

- Reverse, 1st Shift Solenoid Valve - S1 (310) to Control Valve Body (39)

302

1

M5x0.8x28 mm

7 N·m

62 lb in

- Reverse Shift Solenoid Valve - S5 (305) to Control Valve Body (39)

302

1

M5x0.8x28 mm

7 N·m

62 lb in

- 1-2, 2-3, Reverse, Shift Solenoid Valve - S3 (300) to Control Valve Body (39)

301

1

M5x0.8x62 mm

7 N·m

62 lb in

- 2-3, 3-4 Shift Solenoid Valve - S2 (308) to Control Valve Body (39)

307

1

M5x0.8x10 mm

7 N·m

62 lb in

- 3-4, 4-5 Shift Solenoid Valve - S4 (303) to Control Valve Body (39)

302

1

M5x0.8x28 mm

7 N·m

62 lb in