For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the right side lock pillar upper garnish molding. Refer to Lock Pillar Upper Garnish Molding Replacement .

1 | Remote Control Door Lock Receiver

#### Procedure

Refer to Control Module References for programming and set up information.

Tip
Push in on the upper two integral tabs to release the receiver from the body side.