For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Left Rear Differential Mount Nut Notice: Refer to Fastener Notice in the Preface section. Tip Support the rear differential with a jack stand. Tighten
122 N·m (90 lb ft)

2 | Left Rear Differential Mount Bolt (Qty: 2) Tighten 29 N·m (21 lb ft)
3 | Left Rear Differential Mount Bolt (Qty: 2) Tighten 29 N·m (21 lb ft)
4 | Left Rear Differential Mount