For 1990-2009 cars

A clunk noise occurring when accelerating from coast or a standing start may be caused by a worn or damaged wheel drive shaft cross groove joint. The common cause of wheel drive shaft cross groove damage is the loss of lubricating grease and/or the presence of foreign material and contaminates in the joint. This usually occurs as a result of a torn or damaged cross groove joint seal.

Carefully inspect the wheel drive shaft seal for cuts, tears or other damage that may allow the loss of the lubricating grease and/or the entry of contaminates.

After inspection reveals no visual evidence of wear or damage, it may be necessary to remove the wheel drive shaft from the vehicle and manipulate the joint manually. Do not allow the joint to separate from the wheel drive shaft bar. Any binding or impeded movement of the joints may indicate damage which could contribute to the concern.