For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement.
2. Disconnect the electrical connector from the recirculation actuator.
3. Remove the recirculation actuator screws from the HVAC module.
4. Remove the recirculation actuator from the HVAC module.

### Installation Procedure

1. Align the recirculation actuator with the door shaft and rotate into position.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the recirculation actuator screws to the HVAC module.

Tighten the screws to 1.5 N·m (13 lb in).

3. Connect the electrical connector to the recirculation actuator.
4. Cycle the ignition and verify proper operation.
5. Install the instrument panel upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement.