For 1990-2009 cars

#### Special Tools

J 41712 Oil Pressure Switch Socket

### Removal Procedure

1. Turn the ignition OFF.
2. Disconnect the oil pressure sensor electrical connector.
3. Remove the oil pressure sensor (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the oil pressure sensor (1) and tighten to 20 N·m (15 lb ft) .
2. Connect the oil pressure sensor electrical connector.