For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the spare tire.
3. Remove the muffler assembly. Refer to Muffler Replacement .
4. Remove the rear differential assembly. Refer to Differential Replacement .

1 | Clutch Drum Control Module Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 15 N·m (11 lb in).
2 | Clutch Drum Control Module Connector
3 | Clutch Drum Control Module

#### Procedure

Program the differential clutch control module. Refer to Control Module References .