For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Number 2 Seat Replacement .
2. Remove the rear seat head restraint. Refer to Rear Seat Number 2 Head Restraint Replacement .
3. Remove the rear seat head restraint guides. Refer to Rear Seat Number 2 Head Restraint Guide Replacement .
4. Remove the rear seat back recliner handle. Refer to Rear Seat Recliner Handle Replacement .
5. Remove the rear seat outer recliner cover. Refer to Rear Seat Back Recliner Cover Replacement .

1 | Rear Seat No. 2 Back Cover and Pad Refer to Rear Seat Number 2 Back Cushion Cover and Pad Replacement .
2 | Rear Seat No. 2 Back Frame Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Rear Seat No. 2 Back Pivot Bolt Tighten 2 N·m (18 lb in)
4 | Rear Seat No. 2 Back Frame