For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Reposition the positive battery cable boot at the generator terminal.
3. Remove the positive battery cable nut at the generator.
4. Remove the positive battery cable terminal from the generator.
5. Disconnect the engine harness electrical connector from the generator.
6. Remove the drive belt. Refer to Drive Belt Replacement .
7. Remove the idler pulley. Refer to Drive Belt Idler Pulley Replacement .
8. Remove the generator bolts.

Note: When removing the generator from the vehicle, it may be necessary to maneuver the generator to remove it from the vehicle.

9. Remove the generator.

### Installation Procedure

1. Position the generator to the engine.
2. Loosely install the generator bolts.
3. Install the idler pulley. Refer to Drive Belt Idler Pulley Replacement .

Caution: Refer to Fastener Caution in the Preface section.

4. Install the generator bolts in the sequence shown and tighten to 50 N·m (37 lb ft) .
5. Install the drive belt. Refer to Drive Belt Replacement .
6. Connect the engine harness electrical connector to the generator.
7. Install the positive battery cable terminal to the generator.
8. Install the positive battery cable nut at the generator and tighten to 20 N·m (15 lb ft) .
9. Position the positive battery cable boot at the generator terminal.
10. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .