For 1990-2009 cars

### Removal Procedure

1. Pull gently at front of reading lamp cover to disengage retaining clips.
2. Rotate cover rearward until rear attaching hooks are released.
3. Disconnect sunroof switch harness from sunroof switch.
4. Remove sunroof switch fasteners and remove sunroof switch.

### Installation Procedure

1. Install sunroof switch with fasteners.

Tighten
Tighten sunroof switch to 2.5 N·m (22 lb in)

2. Connect sunroof switch harness to sunroof switch.
3. Position front reading lamp cover into rear attaching hooks.
4. Rotate front reading lamp cover into lamp assembly forward, then snap cover into place.
5. Function sunroof switch to ensure proper operation.