For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door outer belt sealing strip retaining screw at the front edge of the door.
2. Remove the rear side door outer belt sealing strip by lifting up on the seal starting at the rear and working forward.

### Installation Procedure

1. Align the outer belt seal fastener location with the hole in the door structure and outer panel retaining tabs.
2. Starting at the rear of the rear side door outer belt sealing strip, push the belt seal down onto the flange until fully seated.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the rear side door outer belt sealing strip retaining screw.

Tighten the screw to 1.5 N·m (13 lb in) .