For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Instrument Panel Compartment Door Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Compartment Door Assembly

#### Procedure

1. Disconnect the instrument panel compartment dampener from the door assembly.
2. Feed the instrument panel compartment door stop out of the opening in the I/P compartment.