For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Front Seat Replacement - Bucket.
2. Remove the recliner handle by pulling firmly forward.
3. Remove the front seat outer adjuster finish cover. Refer to Front Seat Cushion Outer Trim Panel Replacement.

1 | Front Seat Recliner Lever Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Seat Recliner Spring
3 | Front Seat Recliner Lever