For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement.
2. Remove the sixty percent rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Center Rear Seat Belt Retractor To Seat Bolt Caution: Refer to Fastener Caution in the Preface section. Tip Apply GM P/N 12345382 (Canadian P/N 10953489), Permatex® 24200 or equivalent on all seat belt fasteners prior to installation. Tighten
45 N·m (33 lb ft)

2 | Center Rear Seat Belt Retractor To Seat Nut Tip Apply GM P/N 12345382 (Canadian P/N 10953489), Permatex® 24200 or equivalent on all seat belt fasteners prior to installation. Tighten 45 N·m (33 lb ft)
3 | Center Rear Seat Belt Retractor Tip Make sure alignment slots are aligned correctly on reinstallation.