For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove front door extension trim panel. Refer to Upper Extension Trim Panel Replacement.
2. Remove front door handle bezel. Refer to Door Handle Bezel Replacement.
3. Remove front door trim panel. Refer to Front Side Door Trim Panel Replacement.

1 | Front Side Door Locking System Switch Assembly Tip

1. Disconnect electrical connector.
2. Use a flat-bladed tool to pry switch from door handle assembly.