For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove either the LF or RF wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .

1 | Front Fog Lamp Adjuster Screw

#### Procedure

1. Remove the adjuster screw from the fog lamp bracket and lamp assembly.
2. Count the number of turns when removing the adjuster screw for a reference upon installation.
3. Aim the fog lamps after installation. Refer to Fog Lamp Aiming .

2 | Front Fog Lamp Screws (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Front Fog Lamp Assembly Tip Remove the fog lamp assembly from the front fascia bracket.
4 | Fog Lamp Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Rotate the bulb socket counterclockwise from the lamp assembly.